**ALL SAMSUNG CODES**

\*#06# Show IMEI

\*#9999# Show Software Version

\*#0837# Show Software Version (instructions)

\*#0001# Show Serial Parameters

\*#9125# Activates the smiley when charging

\*#0523# LCD Contrast

\*#9998\*228# Battery status (capacity, voltage, temperature)

\*#9998\*246# Program status

\*#9998\*289# Change Alarm Buzzer Frequency

\*#9998\*324# Debug Screens

\*#9998\*364# Watchdog

\*#9998\*377# EEPROM Error Stack - Use side keys to select values

\*#9998\*427# Trace Watchdog

\*#9998\*523# Change LCD contrast

\*#9998\*544# Jig detect

\*#9998\*636# Memory status

\*#9998\*746# SIM File Size

\*#9998\*778# SIM Service Table

\*#9998\*785# RTK (Run Time Kernel) errors - if ok then phn is reset,

info is put in memory error

\*#9998\*786# Run, Last UP, Last DOWN

\*#9998\*837# Software Version

\*#9998\*842# Test Vibrator - Flash the screenlight during 10 sec

and vibration activated

\*#9998\*862# Vocoder Reg - Normal, Earphone or Carkit

\*#9998\*872# Diag

\*#9998\*947# Reset On Fatal Error

\*#9998\*999# Last/Chk

\*#9998\*9266# Yann debug screen (Debug Screens?)

\*#9998\*9999# Software version

\*0001\*s\*f\*t# Changes serial parameters (s=?, f=0.1, t=0.1)

\*0002\*?# unknown

\*0003\*?# unknown

FOR NEW SGH (R210, T100, A300...)

if code is in format \*#9998\*xxx#

try write in this \*#0xxx#

SGH-600

SGH-2100

\*2767\*3855# Full EEPROM Reset (THIS CODE REMMOVES SP-LOCK!

but also changes IMEI to 447967-89-400044-0

\*2767\*2878# Custom EEPROM Reset

SGH E700

\*2767\*688# remove USER CODE and SIMLOCK

SGH V200

Unlocking:

Power on the phone without SIM card and type these codes:

\*2767\*63342# and press green button

\*2767\*3855# and press green button

\*2767\*2878# and press green button

\*2767\*927# and press green button

\*2767\*7822573738# press button

Phone will be unlocked, but all trims are reseted !!!

Mobile phone must be fully charged

SGH S500

Unlocking

\*2767\*MVT# (\*2767\*688#) E2P MVT Reset

\*#SIMLOCK# (\*#7465625#)

" E900 software version: \*#5002\*8376263#

" E900 full reset: \*2767\*3855#